The basic driver is run\_global\_RBF\_TRM in directory main functions.

This driver can run any/all test functiomns except #22,23 (need ADMAT installed).

The best parameters to choose in run\_global\_RBF\_TRM :

gr\_phase2= 1 (does both phases, with smoothing).

Useg=0 (does not use gradient in phase 1).